Table of contents
TECE sanitary modules
TECE sanitary modules
TECEprofil toilet module with Compact
320 cistern, installation height 1120 mm
Toilet module including “easy fit” flush
plate assembly. For fixing to TECEprofil
section tubes or for installation in
metal or wooden stud walls and as a
pre-wall or corner module also suitable
for single block assembly.
Compact 320 cistern for operation from
the front:
- Safety tank made of impact-resistant
plastic, tested according to EN 14055
- Cistern completely pre-assembled
- Cistern connection with R 1/2” outer
thread from above, compatible with
quick-action adapters
- 3-way corner valve shut-off valve with
flush function when filling valve is
fitted
- 7 litre tank volume 6 litre preset
standard flush volume 4.5 litre flush
volume adjustable at any time 3 litre
partial flush with dual-flush system
setting of a 4/2 litre flush volume
optionally possible. Remaining volume
can be used for immediate cleaning
flush.
- Insulated against condensation water
- For TECE flush plates and toilet flush
handle
- Can be used as a single or dual-flush
cistern
- “easy fit” flush plate mounting
- Installation tunnel for service
opening, can be shortened without tools
- Low-noise hydraulic filling valve,
acoustic group 1 to DIN 4109
Module frame:
- self-supporting, powder-coated
- Two M 12 retaining bolts and nuts
- Toilet drain bend DN 90 incl. joint
adapter DN 90/100 made of PP
- Joint adapter also suitable for
horizontal installation
- Toilet connection set DN 90, including
building protection plug
Order-No.: 9300600